Freezer Specs

* 12’ x 14’ x 8’2” Outdoor Walk-In Freezer for cold weather w/non-NSF Floor
* 4.5 HP Condensing Unit, Scroll Compressor, 208-230, 3 Phase
* 13000 BTU Evaporator, 208-230, 1 Phase
* Sloped EPS Foamed Roof with Membrane
* Standard Enclosure Trim Metal
* 36” door
* 4” minimum insulation
* Steel floor
* 5 Year Compressor Warranty

Labor to Include:

Receiving and installing new freezer, setting condensing unit, hanging evaporator, installing refrigerant and condensate piping, Starting and testing unit.

Not to Include:

Demolition of existing unit (in-house).

Electrical (in-house).

Forklift to receive unit (in-house).

Installation approximately 6 – 8 weeks after completion of bid.

Site for install:

Mike Durfee State Prison

1412 Wood St.

Springfield SD 57062

Contact: Rob Caruana rob.caruana@state.sd.us 605-369-4481 cell 605-941-0183

Completion of form and background checks are required for entering the prison.