**RFQ 3892754**

**Addendum 1**

There was a mistake in item 2’s specifications. Here is the corrected specifications:

Item 2 (Xray source)

* UHV compatible.
* 150 mm or 6 inch Z travel.
* ± 12 mm (0.5 inch) XY travel.
* Edge welded bellow, 47.5 (1.87”) mm clearance ID.
* DN 38 (2.75”) CF top and DN 63 (4.5” bottom flanges. Top flange tapped mm, bottom flange clearance holes.
* Full compression length, 4”
* Manual drive.
* Metric scales.
* Horizontal mounting compatible.